 # Delivered to the U.S. Government in Accordance with Contract FA8650-10-C-7080.
 #
 # EXPORT CONTROLLED
 # ECCN#   EAR99  
 # Warning:  This document contains technical data which is controlled under the
 # Bureau of Industry & Security’s Export Administration Regulations and may not be
 # exported or re-exported without authorization by the Bureau of Industry & Security.
 # Diversion contrary to US law is prohibited.
 #
 # (c) 2011 United Technologies Corp.
 # Developed with the sponsorship of the Defense Advanced Research Projects Agency (DARPA).
 #
 # Permission is hereby granted, free of charge, to any person obtaining a copy of this data,
 # including any software or models in source or binary form, as well as any drawings, 
 # specifications, and documentation (collectively "the Data"), to deal in the Data without 
 # restriction, including without limitation the rights to use, copy, modify, merge, publish,
 # distribute, sublicense, and/or sell copies of the Data, and to permit persons to whom the Data
 # is furnished to do so, subject to the following conditions:
 #  
 # The above copyright notice and this permission notice shall be included in all copies or
 # substantial portions of the Data.
 #  
 # THE DATA IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING
 # BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
 # NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS, SPONSORS, DEVELOPERS, CONTRIBUTORS, OR
 # COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION
 # OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE DATA OR THE
 # USE OR OTHER DEALINGS IN THE DATA.

###### HPC$_g:				# High Pressure Compressor
let Nc$_g:=0.9;				# Isentropic Efficiency							
let m$_g:=20;				# Mass Flow (kg/s)
let rc$_g:= 10;  	 		# Pressure Ratio
let To$_g:= 800;	 		# Total Temperature (Kelvin)
let Po$_g:=400000;			# Total Pressure (Pascal)
let W$_g:= -500000; 		# Shaft Power (Watt)
let cp$_g:=1150;			# Specific Heat at Constant Pressure (J/kg/Kelvin)
let gam$_g:=1.35;			# Ratio of Specific Heats 	
let omega$_g:=2000;			# Angular Velocity (Rad/s)

let D_$_g_1:=2000;					# Design Guess
let D_$_g_2:=20;					# Design Guess
let D_$_g_3:=10;					# Design Guess
let D_$_g_4:=0.5;					# Design Guess
let D_$_g_5:=0.9;					# Design Guess
let D_$_g_6:=600;					# Design Guess
let D_$_g_7:=200000;				# Design Guess

let thrust[$_g]:=0;